Ardusub

Q ground control

The raspberry pi acts as a bridge between PC to pixhawk

Use putty to tunnel into the pi, then use qgroundcontrol

Potential disconnecting bug with the pixhawk?

<https://www.intel.com/content/www/us/en/nuc/nuc-replaceable-lids.html>