Documentation here: <http://docs.bluerobotics.com/bar30/#installation>

Barometer has 4 pins that need to be connected to arduino board…

\*This is for the ARDUINO UNO BOARD\*

Red Wire: Plug to power source (3.3V - 5.5V)

Green Wire: Plug into (SCL) a.k.a A5 located on Arduino board

White Wire: Plug into (SDA) a.k.a A4 located on Arduino board

Black Wire: Plug into ground.

Check for specific wiring for different arduino boards here: <https://www.arduino.cc/en/Reference/Wire>