Plug in cameras and pixhawk when Nuc is powered but turned off (Nuc power button should be red).

Order:

1. Remove all ports

2. Plug Power Port into NUC

3. Pixhawk on top USB port of NUC

4. Turn on NUC

-Start Timer...

5. Plug power to Pixhawk

6. Camera A bottom USB port on NUC

7. Camera B micro usb port on NUC

-Wait 1 min 30 sec for pixhawk to arm.

DISCLAIMER:

-If pixhawk does not arm within the minute 40 sec, then ERROR!

Remove Order:

1. Remove power plug first
2. Camera B (micro usb)
3. Pixhawk
4. Camera A (usb)
5. Remove power from pixhawk pin.