**Port configurations for pixhawk and servo communication:**

\*possibly do not need the external battery source\*

Port #1 does not work because of its bent pins.

Port #8 is power source.

Claw works on port #’s: 2, 3, 5, 7, 9, 10, 11

Does not work on: #’s: 1, 4, 6, 12, 13, 14