<http://docs.bluerobotics.com/lumen/>

Current Plan:

Connect the data wire to the pixhawk and connect the power wire from the connections found from the raspberry pi (raspberry pi no longer being used)